**Riser Slitting Tool**

RST-8514

Designed to shave a longitudinal access window in round FTTH riser cables and microducts, this riser slitting tool is perfect for making access windows on cables 8 to 14 mm (0.33” to 0.55”) in diameter without damaging the fibre inside. This tool features the following:

* Lightweight and narrow body can access closely spaced and surface mounted cables
* High carbon steel blade slices through any type of FTTH cable
* Factory-fixed blade requires no adjustments when working with different diameter cables

**Specifications**

|  |  |
| --- | --- |
| **Cut Type** | Slit |
| **Cable Type** | FTTH Riser |
| **Cable Diameter** | 8.5 - 14 mm (0.33" - 0.55") |
| **Dimensions** | 4" x 1.5" x 0.625" (101.6 mm x 38.1 mm x 15.8 mm) |
| **Weight** | 0.201 lbs (91.17g) |
| **UPC No.** | 811490017528 |